{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":25,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":158,"n_cols":6,"rows_kept":158,"cut":false,"hidden":false,"merged":[[133,4,137,4],[133,5,137,5],[139,4,143,4],[139,5,143,5],[145,4,149,4],[145,5,149,5],[151,4,155,4],[151,5,155,5],[145,0,149,0],[145,1,149,1],[151,0,155,0],[151,1,155,1],[151,2,155,2],[151,3,155,3],[145,2,149,2],[145,3,149,3],[121,2,125,2],[121,3,125,3],[139,0,143,0],[139,1,143,1],[139,2,143,2],[139,3,143,3],[133,0,137,0],[133,1,137,1],[133,2,137,2],[133,3,137,3],[61,5,65,5],[67,2,71,2],[67,3,71,3],[67,4,71,4],[67,5,71,5],[115,0,119,0],[115,1,119,1],[115,2,119,2],[115,3,119,3],[109,0,113,0],[109,1,113,1],[109,2,113,2],[109,3,113,3],[109,4,113,4],[109,5,113,5],[115,4,119,4],[115,5,119,5],[1,4,5,4],[1,5,5,5],[1,0,5,0],[1,1,5,1],[1,2,5,2],[1,3,5,3],[13,4,17,4],[13,5,17,5],[19,0,23,0],[19,1,23,1],[19,2,23,2],[19,3,23,3],[19,4,23,4],[19,5,23,5],[13,0,17,0],[13,1,17,1],[7,4,11,4],[7,5,11,5],[31,2,35,2],[31,3,35,3],[31,4,35,4],[31,5,35,5],[13,2,17,2],[13,3,17,3],[7,0,11,0],[7,1,11,1],[7,2,11,2],[7,3,11,3],[25,4,29,4],[25,5,29,5],[31,0,35,0],[31,1,35,1],[25,0,29,0],[25,1,29,1],[25,2,29,2],[25,3,29,3],[49,5,53,5],[55,5,59,5],[49,0,53,0],[55,0,59,0],[49,1,53,1],[55,1,59,1],[49,2,53,2],[55,2,59,2],[37,4,41,4],[37,5,41,5],[43,0,47,0],[43,1,47,1],[43,2,47,2],[43,3,47,3],[43,4,47,4],[43,5,47,5],[37,0,41,0],[37,1,41,1],[37,2,41,2],[37,3,41,3],[61,0,65,0],[61,1,65,1],[67,0,71,0],[67,1,71,1],[61,2,65,2],[61,3,65,3],[49,3,53,3],[55,3,59,3],[49,4,53,4],[55,4,59,4],[61,4,65,4],[73,4,77,4],[73,5,77,5],[79,0,83,0],[79,1,83,1],[79,2,83,2],[79,3,83,3],[79,4,83,4],[79,5,83,5],[73,0,77,0],[73,1,77,1],[73,2,77,2],[73,3,77,3],[85,4,89,4],[85,5,89,5],[91,4,95,4],[91,5,95,5],[103,4,107,4],[103,5,107,5],[85,0,89,0],[85,1,89,1],[85,2,89,2],[85,3,89,3],[97,4,101,4],[97,5,101,5],[91,0,95,0],[91,1,95,1],[91,2,95,2],[91,3,95,3],[157,4,161,4],[157,5,161,5],[157,0,161,0],[157,1,161,1],[157,2,161,2],[157,3,161,3],[97,0,101,0],[97,1,101,1],[103,0,107,0],[103,1,107,1],[103,2,107,2],[103,3,107,3],[97,2,101,2],[97,3,101,3],[121,4,125,4],[121,5,125,5],[127,4,131,4],[127,5,131,5],[121,0,125,0],[121,1,125,1],[127,0,131,0],[127,1,131,1],[127,2,131,2],[127,3,131,3]]}
["Product","Names","Coverage","Application","Characteristics","Product #"]
[null,"Color Boost                         WLP","Up to 120sf                  per gallon","2-3 Coat Application                     Roller                  Sprayer","Water Based                      Wet Look               Matte Finish","1 gallon                       121-393                    5 gallon                     121-396     "]
[]
[]
[]
[]
[]
[null,"WLS                                     CE+","Up to 150sf                   per gallon","2 Coat Application                     Roller                   Sprayer","Water Based                   Wet Look                       Gloss Finish","1 gallon                   121-333                     5 gallon                      121-336"]
[]
[]
[]
[]
[]
[null,"Natural Look                             IN","Up to 120sf                     per gallon","2 Coat Application                     Roller                             Sprayer","Water Based                   Invisible                  Matte Finish","1 gallon                  121-313                                5 gallon                   121-316           "]
[]
[]
[]
[]
[]
[null,"Clear Look                EV","Up to 150sf                 per gallon","1 Coat to Saturation          Roller                   Sprayer","Water Based                 Natural Look                        Satin Finish","1 gallon                   121-303                     5 gallon                      121-306"]
[]
[]
[]
[]
[]
[null,"Nu Look                        Honey ","Up to 150sf                             per gallon","1 Coat to Saturation        Spray only","Water Based              Tinted Colors                  Satin Finish","1 gallon                            121-353                                    5 gallon                                       121-356"]
[]
[]
[]
[]
[]
[null,"Nu Look                       Cognac","Up to 150sf                             per gallon","1 Coat to Saturation        Spray only","Water Based              Tinted Colors                  Satin Finish","1 gallon                         121-323                       5 gallon                                                121-326"]
[]
[]
[]
[]
[]
[null,"Nu Look                    Charcoal","Up to 150sf                             per gallon","1 Coat to Saturation        Spray only","Water Based              Tinted Colors                  Satin Finish","1 gallon                           121-343                                  5 gallon                        121-346"]
[]
[]
[]
[]
[]
[null,"Nu Look                           Brick Red","Up to 150sf                             per gallon","1 Coat to Saturation        Spray only","Water Based              Tinted Colors                  Satin Finish","1 gallon                       121-373                               5 gallon                                     121-376"]
[]
[]
[]
[]
[]
[null,"Brick and Concrete                 WR7                                     Water Repellant","Up to 150sf                         per gallon","1 Coat to Saturation                             Brush, Roll, or Spray","Siloxane Based                     Matte Finish","1 gallon                                   121-383                                   5 gallon                                   121-386"]
[]
[]
[]
[]
[]
[null,"Permeable Joint Stabilizer  JS","Up to 140sf                         per gallon","1 Coat to Saturation                                Spray only","Water Based                                  Satin Finish                                     Natural Look","1 gallon                                          121-413                                    5 gallon                                          121-416"]
[]
[]
[]
[]
[]
[null,"Paver Primer                            Efflorescence Cleaner","Dilution 4:1                 200sf/dilution","Application with Exact Sprayed, Watering Can, or Predilution Tank ","Removes ground in dirt, cement paste, and efflorescence","1 gallon                       121-534                     5 gallon                       121-536"]
[]
[]
[]
[]
[]
[null,"Hardscape Cleaner","Dilution 9:1              800sf/dilution","Application with Exact Sprayed, Watering Can, or Predilution Tank ","Removes ground in dirt and cement paste","1 gallon                 121-503                       5 gallon                         221-506"]
[]
[]
[]
[]
[]
[null,"Paver Restorer","Dilution 1:1                       240sf/dilution","Application with a Watering Can or Predilution Tank ","Removes polymeric sand haze","1 gallon                121-604"]
[]
[]
[]
[]
[]
[null,"Slurry Remover","Dilution 8:1            Approximately                400sf/dilution","Application with a Watering Can or Predilution Tank ","Removes ground in dirt, cement paste, efflorescence, and polymeric sand haze","1 gallon                    221-553                        5 gallon                      221-556"]
[]
[]
[]
[]
[]
[null,"Solvent Based Stripper","Up to 400sf/gallon","Apply and spread with a stiff bristle broom - pressure wash to remove","Removes sealant needs 30-60 mintues to work","5 gallon                     221-547"]
[]
[]
[]
[]
[]
[null,"Eco Stripper",null,"Apply to surface            Sweep & Blow Off             Light Pressure Wash","Removes Sealant                Needs 24-48 hours to work","5 gallon                     221-596"]
[]
[]
[]
[]
[]
[null,"Professional Grade Oil & Grease Remover","Coverage varies ","Apply generously to stains, allow to sit for 4-8 hours, sweeps up in a powder form","Removes penetrated oil and grease stains","Quart                               121-591"]
[]
[]
[]
[]
[]
[null,"Rust Remover","Coverage varies","Apply straight, scrub, and rinse thoroughly","Removes rust, fertilizer, and hard water stains","Quart                                    121-521"]
[]
[]
[]
[]
[]
[null,"Paint, Tar, and Rubber Remover","Coverage varies","Apply, spread evenly, allow 10-15 minutes to work, and rinse thoroughly","Removes paint, tar, rubber, and chewing gum           will dissolve sealant","Quart                                 121-541"]
[]
[]
[]
[]
[]
[null,"Organic Stain Remover","Approximate coverage of 200sf","Dilute in water, apply, lightly scrub, and rinse thoroughly","Removes leaf, mildew, algae, wine, blood, and non greasy food stains","25 oz.                    121-502"]
[]
[]
[]
[]
[]
[null,"RG+ Polymeric Sand","Approximate coverage of 75sf/bag depending upon joint width and depth","Prevents weed growth, insect infestation, and washout","Colors available         Tan                      Granite Gray                        Karbon","50lb. Bag              Tan 191-637                      Granite 191-647                             Karbon 191-667                       "]
[]
[]
[]
[]
[]
[null,"HP2 Polymeric Sand","Approximate coverage of 75sf/bag depending upon joint width and depth","Prevents weed growth, insect infestation, and washout","Colors available         Tan                      Granite Gray                        ","50lb. Bag             Tan 191-037                 Granite 191-047          Karbon 191-067                  "]
[]
[]
[]
[]
[]
[null,"RG+ Concrete Adhesive","Designed for paver and wall block adhesion","Provides a strong, durable bond that resists the elements","Remains flexible","10 oz. tube                   221-791                          28 oz. tube                               221-792"]
[]
[]
[]
[]
[]
[null,"Exact Sprayer","Dilution settings for both Paver Primer and Hardscape Cleaner","Attaches to 1 gallon containers only","Increases productivity by not having to mix cleaners","145-900"]
[]
[]
[]
[]
[]
[null,"Foam Roller","Holds more sealant, applies sealant evenly, and remains spongy","Designed for Water- based sealants","Makes applying sealant easy and quick","145-930"]
[]
[]
[]
[]
[]
[null,"Paver Maid","The ultimate paver care kit to leave behind for your customer","Contains samples of Oil&Grease Remover, PTR, Rust Remover, & Organic Stair Remover","Opens the door for future clean and seal opportunities","121-500"]
[]
[]
[]
[]
[]
[null,"Small Brush for Stain Removal","Acid Resistant",null,"12 brushes per case","145-910"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}